(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1~bpo9+1)
  (general
    (links 75)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 15)
    (tracks 261)
    (zones 0)
    (modules 22)
    (nets 31)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user hide)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VIN)
  (net 2 /VCC)
  (net 3 "Net-(J2-Pad1)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(J2-Pad3)")
  (net 6 "Net-(J2-Pad4)")
  (net 7 "Net-(J2-Pad5)")
  (net 8 "Net-(J2-Pad6)")
  (net 9 "Net-(J2-Pad7)")
  (net 10 "Net-(J2-Pad8)")
  (net 11 "Net-(J3-Pad1)")
  (net 12 "Net-(J3-Pad2)")
  (net 13 "Net-(J3-Pad3)")
  (net 14 "Net-(J3-Pad4)")
  (net 15 "Net-(J3-Pad5)")
  (net 16 "Net-(J3-Pad6)")
  (net 17 "Net-(SW1-Pad2)")
  (net 18 /CLK)
  (net 19 /DIO)
  (net 20 /SDA)
  (net 21 /SCL)
  (net 22 "Net-(SW9-Pad1)")
  (net 23 "Net-(SW9-Pad3)")
  (net 24 /GND)
  (net 25 "Net-(I1-Pad5)")
  (net 26 "Net-(I1-Pad6)")
  (net 27 "Net-(I1-Pad7)")
  (net 28 "Net-(I1-Pad8)")
  (net 29 "Net-(I1-Pad11)")
  (net 30 "Net-(I1-Pad12)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CLK)
    (add_net /DIO)
    (add_net /GND)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /VCC)
    (add_net /VIN)
    (add_net "Net-(I1-Pad11)")
    (add_net "Net-(I1-Pad12)")
    (add_net "Net-(I1-Pad5)")
    (add_net "Net-(I1-Pad6)")
    (add_net "Net-(I1-Pad7)")
    (add_net "Net-(I1-Pad8)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(SW9-Pad1)")
    (add_net "Net-(SW9-Pad3)")
  )
  (module Housings_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 5AE7A440)
    (at 134.62 92.71 90)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 0.635 90) (layer F.SilkS))
    (fp_text value TM1637 (at 3.81 26.035 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /GND))
    (pad 11 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J3-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 14 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad4)"))
    (pad 15 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad5)"))
    (pad 16 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VCC))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad6)"))
    (pad 17 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /DIO))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad7)"))
    (pad 18 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /CLK))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad8)"))
    (pad 19 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(SW9-Pad1)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J3-Pad6)"))
    (pad 20 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(SW9-Pad3)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC4CC02)
    (at 128.27 86.36)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference M3 (at 0 2.54) (layer F.Fab))
    (fp_text value "" (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC4CC05)
    (at 170.18 86.36)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference M3 (at 0 2.54) (layer F.Fab))
    (fp_text value "" (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC4CC09)
    (at 170.18 128.27)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 -2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC4CC0E)
    (at 128.27 128.27)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 -2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE7A453)
    (at 128.27 93.345)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference I1 (at 0 -2.33) (layer F.Fab))
    (fp_text value SerialInput (at -1.905 26.035 90) (layer F.Fab))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(I1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(I1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(I1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(I1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /SDA))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /SCL))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(I1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(I1-Pad12)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE7A43A)
    (at 170.18 93.345)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O1 (at 0 -2.33) (layer F.Fab))
    (fp_text value Output (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(I1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(I1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(I1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(I1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /SDA))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /SCL))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(I1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(I1-Pad12)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5ACCE48B)
    (at 133.985 116.205 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value Select (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /CLK))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /DIO))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 5AFEC9D1)
    (at 134.62 95.885 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Segments (at 0 8.255 180) (layer F.Fab))
    (fp_text user %R (at 0 8.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad8)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5ACCDB30)
    (at 154.94 95.885 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Grids (at 0 6.35 180) (layer F.Fab))
    (fp_text user %R (at 0 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J3-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP0 (layer F.Cu) (tedit 5ACCDFDE)
    (at 160.02 102.87)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (attr smd)
    (fp_text reference SW2 (at 0 0) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 4.25) (layer F.Fab))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQP0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP0 (layer F.Cu) (tedit 5ACCDFDC)
    (at 143.51 102.87)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (attr smd)
    (fp_text reference SW1 (at 0 0) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 4.25) (layer F.Fab))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQP0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP0 (layer F.Cu) (tedit 5ACCDFE2)
    (at 143.51 111.125)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (attr smd)
    (fp_text reference SW3 (at 0 0) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 4.25) (layer F.Fab))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQP0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP0 (layer F.Cu) (tedit 5ACCDFE6)
    (at 160.02 111.125)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (attr smd)
    (fp_text reference SW4 (at 0 0) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 4.25) (layer F.Fab))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad4)"))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad4)"))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQP0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP0 (layer F.Cu) (tedit 5ACCDFEB)
    (at 143.51 119.38)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (attr smd)
    (fp_text reference SW5 (at 0 0) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 4.25) (layer F.Fab))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad5)"))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad5)"))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQP0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP0 (layer F.Cu) (tedit 5ACCDFEE)
    (at 160.02 119.38)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (attr smd)
    (fp_text reference SW6 (at 0 0) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 4.25) (layer F.Fab))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad6)"))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad6)"))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQP0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP0 (layer F.Cu) (tedit 5ACCDFFF)
    (at 143.51 127.635)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (attr smd)
    (fp_text reference SW7 (at 0 0) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad7)"))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad7)"))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQP0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP0 (layer F.Cu) (tedit 5ACCDFFB)
    (at 160.02 127.635)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (attr smd)
    (fp_text reference SW8 (at 0 0) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad8)"))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad8)"))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQP0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5ACCE4A2)
    (at 136.525 118.745 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C1 (at 1.27 0 90) (layer F.Fab))
    (fp_text value 100pF (at 1.25 2.11 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /CLK))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5ACCE497)
    (at 136.525 113.665 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C2 (at 1.27 0 90) (layer F.Fab))
    (fp_text value 100pF (at 1.25 2.11 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /DIO))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_CuK_JS202011CQN_DPDT_Straight (layer F.Cu) (tedit 5AE7A4B9)
    (at 137.795 122.555 270)
    (descr "CuK sub miniature slide switch, JS series, DPDT, right angle, http://www.ckswitches.com/media/1422/js.pdf")
    (tags "switch DPDT")
    (fp_text reference SW9 (at 2.75 -1.6 270) (layer F.Fab))
    (fp_text value SW_SPDT (at 2.54 1.27 270) (layer F.Fab))
    (fp_text user %R (at 2 1.65 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(SW9-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "Net-(SW1-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "Net-(SW9-Pad3)"))
    (pad 4 thru_hole circle (at 0 3.3 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 2.5 3.3 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 5 3.3 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_CuK_JS202011CQN_DPDT_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 5AFEC9A2)
    (at 131.445 103.505)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.Fab))
    (fp_text value Choice (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(I1-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(I1-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(I1-Pad7)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(I1-Pad8)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /SDA))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /SCL))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(I1-Pad11)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(I1-Pad12)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Bank (at 132.715 126.365 90) (layer F.SilkS))
  (gr_text DIGITS (at 161.925 98.425) (layer F.SilkS))
  (gr_text SEGMENTS (at 143.51 98.425) (layer F.SilkS))
  (gr_text 8 (at 165.735 127.635) (layer F.SilkS))
  (gr_text 7 (at 149.225 127.635) (layer F.SilkS))
  (gr_text 6 (at 165.735 119.38) (layer F.SilkS))
  (gr_text 5 (at 149.225 119.38) (layer F.SilkS))
  (gr_text 4 (at 165.735 111.125) (layer F.SilkS))
  (gr_text 3 (at 149.225 111.125) (layer F.SilkS))
  (gr_text 2 (at 165.735 102.87) (layer F.SilkS))
  (gr_text 1 (at 149.225 102.87) (layer F.SilkS))
  (gr_text DIO (at 133.985 110.49 90) (layer F.SilkS))
  (gr_text CLK (at 133.985 119.38 90) (layer F.SilkS))
  (gr_text "TM1637 v1.1\nhttp://nickthecoder.co.uk" (at 163.83 125.73) (layer B.SilkS))
  (zone (net 0) (net_name "") (layer Edge.Cuts) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.001)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.99 132.08) (xy 124.46 132.08) (xy 124.46 82.55) (xy 173.99 82.55)
      )
    )
  )
  (zone (net 24) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.72 130.81) (xy 125.73 130.81) (xy 125.73 83.82) (xy 172.72 83.82)
      )
    )
  )
)
