(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1~bpo9+1)
  (general
    (links 62)
    (no_connects 0)
    (area 58.42 31.115 158.115001 80.645001)
    (thickness 1.6)
    (drawings 52)
    (tracks 338)
    (zones 0)
    (modules 11)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /A5)
  (net 2 /A4)
  (net 3 /A3)
  (net 4 /A2)
  (net 5 /A1)
  (net 6 /A0)
  (net 7 /VCC)
  (net 8 /VIN)
  (net 9 /GND)
  (net 10 /A6)
  (net 11 /A7)
  (net 12 /B7)
  (net 13 /B6)
  (net 14 /A9)
  (net 15 /A10)
  (net 16 /B0)
  (net 17 /B1)
  (net 18 /B8)
  (net 19 /B9)
  (net 20 /B10)
  (net 21 /B11)
  (net 22 /B12)
  (net 23 /A8)
  (net 24 /A11)
  (net 25 /A12)
  (net 26 /A15)
  (net 27 /C15)
  (net 28 /C14)
  (net 29 /C13)
  (net 30 /B13)
  (net 31 /B14)
  (net 32 /B15)
  (net 33 /B3)
  (net 34 /B4)
  (net 35 /B5)
  (net 36 /5V)
  (net 37 /RESET)
  (net 38 /VBAT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /5V)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /B0)
    (add_net /B1)
    (add_net /B10)
    (add_net /B11)
    (add_net /B12)
    (add_net /B13)
    (add_net /B14)
    (add_net /B15)
    (add_net /B3)
    (add_net /B4)
    (add_net /B5)
    (add_net /B6)
    (add_net /B7)
    (add_net /B8)
    (add_net /B9)
    (add_net /C13)
    (add_net /C14)
    (add_net /C15)
    (add_net /GND)
    (add_net /RESET)
    (add_net /VBAT)
    (add_net /VCC)
    (add_net /VIN)
  )
  (module ePlayPretty:bluePill (layer F.Cu) (tedit 5ACA5DCF)
    (at 69.215 55.88 90)
    (descr http://wiki.stm32duino.com/images/a/ae/Bluepillpinout.gif)
    (fp_text reference U1 (at 0 6.985 90) (layer F.Fab))
    (fp_text value BluePill (at 0 21.082 180) (layer F.Fab))
    (fp_text user USB (at 0 0.635 90) (layer F.SilkS))
    (pad 20 thru_hole circle (at 7.62 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 19 thru_hole circle (at 7.62 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 18 thru_hole circle (at 7.62 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 17 thru_hole circle (at 7.62 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 /RESET))
    (pad 16 thru_hole circle (at 7.62 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /B11))
    (pad 15 thru_hole circle (at 7.62 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /B10))
    (pad 14 thru_hole circle (at 7.62 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /B1))
    (pad 13 thru_hole circle (at 7.62 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /B0))
    (pad 12 thru_hole circle (at 7.62 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /A7))
    (pad 11 thru_hole circle (at 7.62 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /A6))
    (pad 10 thru_hole circle (at 7.62 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad 9 thru_hole circle (at 7.62 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad 8 thru_hole circle (at 7.62 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /A3))
    (pad 7 thru_hole circle (at 7.62 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /A2))
    (pad 6 thru_hole circle (at 7.62 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /A1))
    (pad 5 thru_hole circle (at 7.62 40.64 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /A0))
    (pad 4 thru_hole circle (at 7.62 43.18 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /C15))
    (pad 3 thru_hole circle (at 7.62 45.72 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /C14))
    (pad 2 thru_hole circle (at 7.62 48.26 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /C13))
    (pad 1 thru_hole circle (at 7.62 50.8 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 /VBAT))
    (pad 21 thru_hole circle (at -7.62 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /B12))
    (pad 22 thru_hole circle (at -7.62 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /B13))
    (pad 23 thru_hole circle (at -7.62 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /B14))
    (pad 24 thru_hole circle (at -7.62 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /B15))
    (pad 25 thru_hole circle (at -7.62 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /A8))
    (pad 26 thru_hole circle (at -7.62 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /A9))
    (pad 27 thru_hole circle (at -7.62 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /A10))
    (pad 28 thru_hole circle (at -7.62 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /A11))
    (pad 29 thru_hole circle (at -7.62 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /A12))
    (pad 30 thru_hole circle (at -7.62 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /A15))
    (pad 31 thru_hole circle (at -7.62 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /B3))
    (pad 32 thru_hole circle (at -7.62 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /B4))
    (pad 33 thru_hole circle (at -7.62 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 /B5))
    (pad 34 thru_hole circle (at -7.62 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /B6))
    (pad 35 thru_hole circle (at -7.62 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /B7))
    (pad 36 thru_hole circle (at -7.62 40.64 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /B8))
    (pad 37 thru_hole circle (at -7.62 43.18 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /B9))
    (pad 38 thru_hole circle (at -7.62 45.72 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /5V))
    (pad 39 thru_hole circle (at -7.62 48.26 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 40 thru_hole circle (at -7.62 50.8 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /VCC))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE96CE8)
    (at 147.32 76.835 270)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O1 (at 0 -2.33 270) (layer F.Fab))
    (fp_text value SerialOutput (at 0 34.29 360) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A6))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A7))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /B7))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /B6))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /A9))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /A10))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE98086)
    (at 154.305 41.91)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O2 (at 0 -2.33) (layer F.Fab))
    (fp_text value Output (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /C13))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /C14))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /C15))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /B0))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /B1))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /B3))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /B4))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /B5))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE96CF4)
    (at 119.38 34.925 90)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O3 (at 0 -2.33 90) (layer F.Fab))
    (fp_text value Output (at 0 3.81 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A7))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A6))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /A3))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A2))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A1))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A0))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5ACA5EEE)
    (at 154.305 34.925)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference X (at 0 0) (layer F.Fab))
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC36F82)
    (at 154.305 76.835)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.Fab))
    (fp_text value M3 (at 0 -2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC36FB5)
    (at 62.23 76.835)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.Fab))
    (fp_text value M3 (at 0 -2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5ACA5F07)
    (at 62.23 34.925)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference X (at 0 0) (layer F.Fab))
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE96D00)
    (at 69.85 34.925 90)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O4 (at 0 -2.33 90) (layer F.Fab))
    (fp_text value Output (at 0.635 25.4 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /B12))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /B13))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /A11))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /A12))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /A15))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /A8))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /B8))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /B9))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE96CDA)
    (at 97.79 76.835 270)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O5 (at 0 -2.33 270) (layer F.Fab))
    (fp_text value SerialOutput (at 0 -7.62 360) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /B13))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /B14))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /B15))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /B12))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /B11))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /B10))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A2))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /A3))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 5AFAA4C2)
    (at 132.715 63.5 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.Fab))
    (fp_text value Power (at -1.905 10.16 180) (layer F.Fab))
    (fp_text user %R (at 0 5.08 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /VBAT))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /RESET))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text RESET (at 142.875 61.595 90) (layer F.SilkS))
  (gr_text GND (at 140.335 61.595 90) (layer F.SilkS))
  (gr_text VCC (at 137.795 61.595 90) (layer F.SilkS))
  (gr_text VBAT (at 135.255 61.595 90) (layer F.SilkS))
  (gr_text 5V (at 132.715 61.595 90) (layer F.SilkS))
  (gr_text "(5V tolerant)" (at 92.075 42.545) (layer F.SilkS))
  (gr_text B12 (at 80.01 37.465 90) (layer F.SilkS))
  (gr_text B5 (at 152.4 69.85) (layer F.SilkS))
  (gr_text B4 (at 152.4 67.31) (layer F.SilkS))
  (gr_text A0 (at 147.32 37.465 90) (layer F.SilkS))
  (gr_text A1 (at 144.78 37.465 90) (layer F.SilkS))
  (gr_text "(TX2) A2" (at 142.24 37.465 90) (layer F.SilkS))
  (gr_text "(RX2) A3" (at 139.7 37.465 90) (layer F.SilkS))
  (gr_text "(Serial 1 #4) A4" (at 137.16 37.465 90) (layer F.SilkS))
  (gr_text "(SCK1) A5" (at 134.62 37.465 90) (layer F.SilkS))
  (gr_text "(MISO1) A6" (at 132.08 37.465 90) (layer F.SilkS))
  (gr_text "(MOSI1) A7" (at 129.54 37.465 90) (layer F.SilkS))
  (gr_text "(SCK2) B13" (at 82.55 37.465 90) (layer F.SilkS))
  (gr_text B9 (at 97.79 37.465 90) (layer F.SilkS))
  (gr_text B8 (at 95.25 37.465 90) (layer F.SilkS))
  (gr_text A8 (at 92.71 37.465 90) (layer F.SilkS))
  (gr_text A15 (at 90.17 37.465 90) (layer F.SilkS))
  (gr_text A12 (at 87.63 37.465 90) (layer F.SilkS))
  (gr_text A11 (at 85.09 37.465 90) (layer F.SilkS))
  (gr_text "SCK2 (B13)" (at 87.63 74.295 90) (layer F.SilkS))
  (gr_text "MISO2 (B14)" (at 85.09 74.295 90) (layer F.SilkS))
  (gr_text "MOSI2 (B15)" (at 82.55 74.295 90) (layer F.SilkS))
  (gr_text B12 (at 80.01 74.295 90) (layer F.SilkS))
  (gr_text "SDA2 (B11)" (at 77.47 74.295 90) (layer F.SilkS))
  (gr_text "SCL2 (B10)" (at 74.93 74.295 90) (layer F.SilkS))
  (gr_text "TX2 (A2)" (at 72.39 74.295 90) (layer F.SilkS))
  (gr_text "RX2 (A3)" (at 69.85 74.295 90) (layer F.SilkS))
  (gr_text "SCK1 (A5)" (at 137.16 74.295 90) (layer F.SilkS))
  (gr_text "MISO1 (A6)" (at 134.62 74.295 90) (layer F.SilkS))
  (gr_text "MOSI1 (A7)" (at 132.08 74.295 90) (layer F.SilkS))
  (gr_text A4 (at 129.54 74.295 90) (layer F.SilkS))
  (gr_text "SDA1 (B7)" (at 127 74.295 90) (layer F.SilkS))
  (gr_text "SCL1 (B6)" (at 124.46 74.295 90) (layer F.SilkS))
  (gr_text "TX1 (A9)" (at 121.92 74.295 90) (layer F.SilkS))
  (gr_text "RX1 (A10)" (at 119.38 74.295 90) (layer F.SilkS))
  (gr_text C15 (at 152.4 57.15) (layer F.SilkS))
  (gr_text C14 (at 152.4 54.61) (layer F.SilkS))
  (gr_text C13 (at 152.4 52.07) (layer F.SilkS))
  (gr_text B3 (at 152.4 64.77) (layer F.SilkS))
  (gr_text OTHER (at 73.66 38.735) (layer F.SilkS))
  (gr_text ANALOG (at 123.19 38.735) (layer F.SilkS))
  (gr_text "SERIAL 1" (at 144.145 73.66) (layer F.SilkS))
  (gr_text "SERIAL 2" (at 94.615 73.66) (layer F.SilkS))
  (gr_text "Blue Pill v1.1\nnickthecoder.co.uk" (at 81.915 55.88) (layer F.SilkS))
  (gr_text B1 (at 152.4 62.23) (layer F.SilkS))
  (gr_text B0 (at 152.4 59.69) (layer F.SilkS))
  (gr_text DIGITAL (at 150.495 45.085 90) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer Edge.Cuts) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.001)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.115 80.645) (xy 58.42 80.645) (xy 58.42 31.115) (xy 158.115 31.115)
      )
    )
  )
  (zone (net 9) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.845 79.375) (xy 59.69 79.375) (xy 59.69 32.385) (xy 156.845 32.385)
      )
    )
  )
)
