(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1~bpo9+1)
  (general
    (links 233)
    (no_connects 13)
    (area 58.42 27.305 167.71 130.810001)
    (thickness 1.6)
    (drawings 93)
    (tracks 641)
    (zones 0)
    (modules 59)
    (nets 90)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.5)
    (user_trace_width 0.5)
    (user_trace_width 0.5)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEF77F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/nick/projects/eplayground/pcb/combined2/))
  )
  (net 0 "")
  (net 1 /A5)
  (net 2 /A4)
  (net 3 /A3)
  (net 4 /A2)
  (net 5 /A1)
  (net 6 /A0)
  (net 7 /VCC)
  (net 8 /VIN)
  (net 9 /GND)
  (net 10 /A6)
  (net 11 /A7)
  (net 12 /B7)
  (net 13 /B6)
  (net 14 /A9)
  (net 15 /A10)
  (net 16 /B0)
  (net 17 /B1)
  (net 18 /B8)
  (net 19 /B9)
  (net 20 /B10)
  (net 21 /B11)
  (net 22 /B12)
  (net 23 /A8)
  (net 24 /A11)
  (net 25 /A12)
  (net 26 /A15)
  (net 27 /C15)
  (net 28 /C14)
  (net 29 /C13)
  (net 30 /B13)
  (net 31 /B14)
  (net 32 /B15)
  (net 33 /B3)
  (net 34 /B4)
  (net 35 /B5)
  (net 36 /5V)
  (net 37 /RESET)
  (net 38 /VBAT)
  (net 39 Earth)
  (net 40 /L0)
  (net 41 /L1)
  (net 42 /L2)
  (net 43 /L3)
  (net 44 /L4)
  (net 45 /L5)
  (net 46 /L6)
  (net 47 /L7)
  (net 48 "Net-(H4-Pad1)")
  (net 49 "Net-(H4-Pad2)")
  (net 50 "Net-(H4-Pad3)")
  (net 51 "Net-(H4-Pad4)")
  (net 52 "Net-(H4-Pad5)")
  (net 53 "Net-(H4-Pad6)")
  (net 54 "Net-(H4-Pad7)")
  (net 55 "Net-(H4-Pad8)")
  (net 56 "Net-(I2-Pad5)")
  (net 57 "Net-(I2-Pad6)")
  (net 58 "Net-(I2-Pad7)")
  (net 59 "Net-(I2-Pad8)")
  (net 60 "Net-(I2-Pad9)")
  (net 61 "Net-(I2-Pad10)")
  (net 62 "Net-(I2-Pad11)")
  (net 63 "Net-(I2-Pad12)")
  (net 64 "Net-(J12-Pad1)")
  (net 65 "Net-(J12-Pad2)")
  (net 66 "Net-(J12-Pad3)")
  (net 67 "Net-(J12-Pad4)")
  (net 68 "Net-(J12-Pad5)")
  (net 69 "Net-(J12-Pad6)")
  (net 70 "Net-(J12-Pad7)")
  (net 71 "Net-(J12-Pad8)")
  (net 72 /D13)
  (net 73 /D12)
  (net 74 /D11)
  (net 75 /D10)
  (net 76 /D1)
  (net 77 /D0)
  (net 78 /D2)
  (net 79 /D3)
  (net 80 /D4)
  (net 81 /D5)
  (net 82 /D6)
  (net 83 /D7)
  (net 84 /D8)
  (net 85 /D9)
  (net 86 /AREF)
  (net 87 /3V3)
  (net 88 /Reset1)
  (net 89 /Reset2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V3)
    (add_net /5V)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /AREF)
    (add_net /B0)
    (add_net /B1)
    (add_net /B10)
    (add_net /B11)
    (add_net /B12)
    (add_net /B13)
    (add_net /B14)
    (add_net /B15)
    (add_net /B3)
    (add_net /B4)
    (add_net /B5)
    (add_net /B6)
    (add_net /B7)
    (add_net /B8)
    (add_net /B9)
    (add_net /C13)
    (add_net /C14)
    (add_net /C15)
    (add_net /D0)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /GND)
    (add_net /L0)
    (add_net /L1)
    (add_net /L2)
    (add_net /L3)
    (add_net /L4)
    (add_net /L5)
    (add_net /L6)
    (add_net /L7)
    (add_net /RESET)
    (add_net /Reset1)
    (add_net /Reset2)
    (add_net /VBAT)
    (add_net /VCC)
    (add_net /VIN)
    (add_net Earth)
    (add_net "Net-(H4-Pad1)")
    (add_net "Net-(H4-Pad2)")
    (add_net "Net-(H4-Pad3)")
    (add_net "Net-(H4-Pad4)")
    (add_net "Net-(H4-Pad5)")
    (add_net "Net-(H4-Pad6)")
    (add_net "Net-(H4-Pad7)")
    (add_net "Net-(H4-Pad8)")
    (add_net "Net-(I2-Pad10)")
    (add_net "Net-(I2-Pad11)")
    (add_net "Net-(I2-Pad12)")
    (add_net "Net-(I2-Pad5)")
    (add_net "Net-(I2-Pad6)")
    (add_net "Net-(I2-Pad7)")
    (add_net "Net-(I2-Pad8)")
    (add_net "Net-(I2-Pad9)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J12-Pad2)")
    (add_net "Net-(J12-Pad3)")
    (add_net "Net-(J12-Pad4)")
    (add_net "Net-(J12-Pad5)")
    (add_net "Net-(J12-Pad6)")
    (add_net "Net-(J12-Pad7)")
    (add_net "Net-(J12-Pad8)")
  )
  (module ePlayPretty:bluePill (layer F.Cu) (tedit 5ACA5DCF)
    (at 69.215 55.88 90)
    (descr http://wiki.stm32duino.com/images/a/ae/Bluepillpinout.gif)
    (fp_text reference U1 (at 0 6.985 90) (layer F.Fab))
    (fp_text value BluePill (at 0 21.082 180) (layer F.Fab))
    (fp_text user USB (at 0 0.635 90) (layer F.SilkS))
    (pad 20 thru_hole circle (at 7.62 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 19 thru_hole circle (at 7.62 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 18 thru_hole circle (at 7.62 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 17 thru_hole circle (at 7.62 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 /RESET))
    (pad 16 thru_hole circle (at 7.62 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /B11))
    (pad 15 thru_hole circle (at 7.62 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /B10))
    (pad 14 thru_hole circle (at 7.62 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /B1))
    (pad 13 thru_hole circle (at 7.62 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /B0))
    (pad 12 thru_hole circle (at 7.62 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /A7))
    (pad 11 thru_hole circle (at 7.62 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /A6))
    (pad 10 thru_hole circle (at 7.62 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad 9 thru_hole circle (at 7.62 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad 8 thru_hole circle (at 7.62 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /A3))
    (pad 7 thru_hole circle (at 7.62 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /A2))
    (pad 6 thru_hole circle (at 7.62 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /A1))
    (pad 5 thru_hole circle (at 7.62 40.64 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /A0))
    (pad 4 thru_hole circle (at 7.62 43.18 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /C15))
    (pad 3 thru_hole circle (at 7.62 45.72 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /C14))
    (pad 2 thru_hole circle (at 7.62 48.26 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /C13))
    (pad 1 thru_hole circle (at 7.62 50.8 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 /VBAT))
    (pad 21 thru_hole circle (at -7.62 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /B12))
    (pad 22 thru_hole circle (at -7.62 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /B13))
    (pad 23 thru_hole circle (at -7.62 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /B14))
    (pad 24 thru_hole circle (at -7.62 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /B15))
    (pad 25 thru_hole circle (at -7.62 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /A8))
    (pad 26 thru_hole circle (at -7.62 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /A9))
    (pad 27 thru_hole circle (at -7.62 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /A10))
    (pad 28 thru_hole circle (at -7.62 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /A11))
    (pad 29 thru_hole circle (at -7.62 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /A12))
    (pad 30 thru_hole circle (at -7.62 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /A15))
    (pad 31 thru_hole circle (at -7.62 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /B3))
    (pad 32 thru_hole circle (at -7.62 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /B4))
    (pad 33 thru_hole circle (at -7.62 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 /B5))
    (pad 34 thru_hole circle (at -7.62 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /B6))
    (pad 35 thru_hole circle (at -7.62 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /B7))
    (pad 36 thru_hole circle (at -7.62 40.64 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /B8))
    (pad 37 thru_hole circle (at -7.62 43.18 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /B9))
    (pad 38 thru_hole circle (at -7.62 45.72 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /5V))
    (pad 39 thru_hole circle (at -7.62 48.26 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 40 thru_hole circle (at -7.62 50.8 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /VCC))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE96CE8)
    (at 147.32 76.835 270)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O1 (at 0 -2.33 270) (layer F.Fab))
    (fp_text value SerialOutput (at 0 34.29 360) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A6))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A7))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /B7))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /B6))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /A9))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /A10))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE98086)
    (at 154.305 41.91)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O2 (at 0 -2.33) (layer F.Fab))
    (fp_text value Output (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /C13))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /C14))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /C15))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /B0))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /B1))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /B3))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /B4))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /B5))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE96CF4)
    (at 119.38 34.925 90)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O3 (at 0 -2.33 90) (layer F.Fab))
    (fp_text value Output (at 0 3.81 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A7))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A6))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /A3))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A2))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A1))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A0))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5ACA5EEE)
    (at 154.305 34.925)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference X (at 0 0) (layer F.Fab))
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC36F82)
    (at 154.305 76.835)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.Fab))
    (fp_text value M3 (at 0 -2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC36FB5)
    (at 62.23 76.835)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.Fab))
    (fp_text value M3 (at 0 -2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5ACA5F07)
    (at 62.23 34.925)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference X (at 0 0) (layer F.Fab))
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE96D00)
    (at 69.85 34.925 90)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O4 (at 0 -2.33 90) (layer F.Fab))
    (fp_text value Output (at 0.635 25.4 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /B12))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /B13))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /A11))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /A12))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /A15))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /A8))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /B8))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /B9))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE96CDA)
    (at 97.79 76.835 270)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O5 (at 0 -2.33 270) (layer F.Fab))
    (fp_text value SerialOutput (at 0 -7.62 360) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /B13))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /B14))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /B15))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /B12))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /B11))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /B10))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A2))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /A3))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 5AC79602)
    (at 102.235 106.68)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J3 (at 1.78 0 270) (layer B.SilkS) hide)
    (fp_text value GS2 (at -1.8 0 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(H4-Pad3)"))
    (pad 2 smd rect (at 0 -0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 42 /L2))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5ACF1C6A)
    (at 104.14 92.075)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O2 (at 0 -2.33) (layer F.Fab) hide)
    (fp_text value Output (at 0 30.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(H4-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(H4-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(H4-Pad3)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(H4-Pad4)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(H4-Pad5)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(H4-Pad6)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(H4-Pad7)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(H4-Pad8)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5AC794F5)
    (at 64.135 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference H1 (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Headers8L (at 0 -20.11 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /L0))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /L1))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /L2))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /L3))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /L4))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /L5))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /L6))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /L7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5ACF1FC7)
    (at 66.675 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at -7.62 -17.145 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer B.Cu) (tedit 5ACF1ADD)
    (at 66.675 97.155 270)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 270) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at -0.635 -17.78 540) (layer B.Fab) hide)
    (fp_text user %R (at 0 -16.51 540) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer B.Cu) (tedit 5ACF1ADD)
    (at 66.675 99.695 270)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 270) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at -0.635 -17.78 540) (layer B.Fab) hide)
    (fp_text user %R (at 0 -16.51 540) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer B.Cu) (tedit 5ACF207F)
    (at 66.675 89.535 270)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J11 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value Conn_01x14 (at 0 -35.35 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -16.51 360) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC4CC02)
    (at 62.23 85.09)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference M3 (at 0 2.54) (layer F.Fab))
    (fp_text value "" (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC4CC05)
    (at 104.14 85.09)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference M3 (at 0 2.54) (layer F.Fab))
    (fp_text value "" (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC4CC09)
    (at 104.14 127)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 -2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC4CC0E)
    (at 62.23 127)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 -2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AC79C00)
    (at 61.595 92.075)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference I1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Input (at 0 30.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /L0))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /L1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /L2))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /L3))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /L4))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /L5))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /L6))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /L7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AC79C04)
    (at 69.215 84.455 90)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference I2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Input (at 0 30.27 90) (layer F.Fab))
    (fp_text user %R (at 0 13.97 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(I2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(I2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(I2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(I2-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(I2-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(I2-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(I2-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(I2-Pad12)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5ACF1C7B)
    (at 97.155 127.635 270)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O1 (at 0 -2.33 270) (layer F.Fab) hide)
    (fp_text value Output (at 0 30.27 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(J12-Pad8)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(J12-Pad7)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J12-Pad6)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(J12-Pad5)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(J12-Pad4)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(J12-Pad3)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(J12-Pad2)"))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(J12-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5ACF1FBC)
    (at 97.155 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at 9.525 -16.51 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5AC78DC7)
    (at 81.915 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at 0 -20.11 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5AC78DCA)
    (at 79.375 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at 0 -20.11 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5AC78DD3)
    (at 89.535 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at 0 -20.11 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5AC78DD5)
    (at 86.995 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at 0 -20.11 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5ACF1FC5)
    (at 71.755 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at -10.16 -17.78 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5AC790FB)
    (at 76.835 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at 0 -20.11 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5AC794DC)
    (at 99.695 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference H4 (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Headers8 (at 0 -20.11 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(H4-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(H4-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(H4-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(H4-Pad4)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(H4-Pad5)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(H4-Pad6)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(H4-Pad7)"))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(H4-Pad8)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 5AC795C9)
    (at 102.235 101.6)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J1 (at 1.78 0 270) (layer B.SilkS) hide)
    (fp_text value GS2 (at -1.8 0 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(H4-Pad1)"))
    (pad 2 smd rect (at 0 -0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 40 /L0))
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 5ACF1994)
    (at 106.045 104.14)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J2 (at -1.905 0 270) (layer B.SilkS) hide)
    (fp_text value GS2 (at -1.8 0 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(H4-Pad2)"))
    (pad 2 smd rect (at 0 -0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 41 /L1))
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 5ACF1997)
    (at 106.045 109.22)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J4 (at -1.905 -0.635 270) (layer B.SilkS) hide)
    (fp_text value GS2 (at -1.8 0 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(H4-Pad4)"))
    (pad 2 smd rect (at 0 -0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 43 /L3))
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 5AC795F5)
    (at 102.235 111.76)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J5 (at 1.78 0 270) (layer B.SilkS) hide)
    (fp_text value GS2 (at -1.8 0 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(H4-Pad5)"))
    (pad 2 smd rect (at 0 -0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 44 /L4))
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 5ACF1999)
    (at 106.045 114.3)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J6 (at -1.905 0 270) (layer B.SilkS) hide)
    (fp_text value GS2 (at -1.8 0 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(H4-Pad6)"))
    (pad 2 smd rect (at 0 -0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 45 /L5))
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 5AC795F0)
    (at 102.235 116.84)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J7 (at 1.78 0 270) (layer B.SilkS) hide)
    (fp_text value GS2 (at -1.8 0 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(H4-Pad7)"))
    (pad 2 smd rect (at 0 -0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 46 /L6))
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 5ACF199C)
    (at 106.045 119.38)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J8 (at -1.905 0 270) (layer B.SilkS) hide)
    (fp_text value GS2 (at -1.8 0 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(H4-Pad8)"))
    (pad 2 smd rect (at 0 -0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 47 /L7))
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5AC794EC)
    (at 84.455 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at 0 -20.11 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5ACF1FCA)
    (at 74.295 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at -5.08 -18.415 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer B.Cu) (tedit 5ACF2077)
    (at 66.675 94.615 270)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J9 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value Conn_01x14 (at 0 -35.35 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -16.51 360) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Earth))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer B.Cu) (tedit 5ACF207B)
    (at 66.675 92.075 270)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J10 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value Conn_01x14 (at 0 -35.35 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -16.51 360) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5AC79CD2)
    (at 92.075 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at 0 -20.11 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5ACF1FBF)
    (at 94.615 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at 5.08 -16.51 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5ACF1FC7)
    (at 69.215 102.235 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at -7.62 -17.145 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5ACF1AD8)
    (at 69.215 125.095 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J12 (at 0 2.33 270) (layer B.Fab) hide)
    (fp_text value Conn_01x08 (at 0 -20.11 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 540) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(J12-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(J12-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(J12-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(J12-Pad4)"))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(J12-Pad5)"))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J12-Pad6)"))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(J12-Pad7)"))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(J12-Pad8)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5ACF190F)
    (at 79.375 86.995 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J13 (at 0 2.33 270) (layer B.Fab) hide)
    (fp_text value Conn_01x08 (at 0 -20.11 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89 540) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(I2-Pad5)"))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(I2-Pad6)"))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(I2-Pad7)"))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(I2-Pad8)"))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(I2-Pad9)"))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(I2-Pad10)"))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(I2-Pad11)"))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(I2-Pad12)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer B.Cu) (tedit 5ACF1ADD)
    (at 66.675 122.555 270)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference REF** (at 0 2.33 270) (layer B.Fab) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at -0.635 -17.78 540) (layer B.Fab) hide)
    (fp_text user %R (at 0 -16.51 540) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE77EE6)
    (at 119.38 85.09 90)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O1 (at 0 -2.33 90) (layer F.Fab))
    (fp_text value SerialOutput (at 2.54 17.145 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 /D13))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 /D12))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 /D11))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 /D10))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 /D1))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 /D0))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE77EFD)
    (at 154.305 92.075)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O2 (at 0 -2.33) (layer F.Fab))
    (fp_text value Output (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 /D2))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 /D3))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 /D4))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 /D5))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 /D6))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 /D7))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 /D8))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 /D9))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE77EF3)
    (at 147.32 127 270)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O3 (at 0 -2.33 270) (layer F.Fab))
    (fp_text value Output (at 0 30.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A7))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A6))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /A3))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A2))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A1))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A0))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AE88C50)
    (at 154.305 85.09)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference X (at 0 0) (layer F.Fab))
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC36F82)
    (at 154.305 127)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.Fab))
    (fp_text value M3 (at 0 -2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC36FB5)
    (at 112.395 127)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.Fab))
    (fp_text value M3 (at 0 -2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AE88C5A)
    (at 112.395 85.09)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference X (at 0 0) (layer F.Fab))
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Arduino:Arduino_Nano (layer F.Cu) (tedit 5A860395)
    (at 106.68 108.585 270)
    (descr https://store.arduino.cc/arduino-nano)
    (fp_text reference XA1 (at 6.604 1.016 270) (layer F.Fab))
    (fp_text value Arduino_Nano_Socket (at 0 -21.082 360) (layer F.Fab))
    (fp_text user USB (at 0 0.635 270) (layer F.Fab))
    (fp_text user 3.3V (at 6.35 -6.35 360) (layer F.Fab))
    (fp_text user ICSP (at 0 -40.64 270) (layer F.Fab))
    (pad VIN thru_hole circle (at 7.62 -39.37 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad GND2 thru_hole circle (at 7.62 -36.83 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad RST2 thru_hole circle (at 7.62 -34.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 89 /Reset2))
    (pad 5V thru_hole circle (at 7.62 -31.75 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad A7 thru_hole circle (at 7.62 -29.21 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /A7))
    (pad A6 thru_hole circle (at 7.62 -26.67 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /A6))
    (pad A5 thru_hole circle (at 7.62 -24.13 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad A4 thru_hole circle (at 7.62 -21.59 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad A3 thru_hole circle (at 7.62 -19.05 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /A3))
    (pad A2 thru_hole circle (at 7.62 -16.51 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /A2))
    (pad A1 thru_hole circle (at 7.62 -13.97 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /A1))
    (pad A0 thru_hole circle (at 7.62 -11.43 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /A0))
    (pad AREF thru_hole circle (at 7.62 -8.89 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 86 /AREF))
    (pad 3V3 thru_hole circle (at 7.62 -6.35 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 87 /3V3))
    (pad D13 thru_hole circle (at 7.62 -3.81 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 /D13))
    (pad D12 thru_hole circle (at -7.62 -3.81 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 /D12))
    (pad D11 thru_hole circle (at -7.62 -6.35 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 /D11))
    (pad D10 thru_hole circle (at -7.62 -8.89 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 /D10))
    (pad D9 thru_hole circle (at -7.62 -11.43 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 85 /D9))
    (pad D8 thru_hole circle (at -7.62 -13.97 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 84 /D8))
    (pad D7 thru_hole circle (at -7.62 -16.51 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 83 /D7))
    (pad D6 thru_hole circle (at -7.62 -19.05 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 82 /D6))
    (pad D5 thru_hole circle (at -7.62 -21.59 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 81 /D5))
    (pad D4 thru_hole circle (at -7.62 -24.13 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 /D4))
    (pad D3 thru_hole circle (at -7.62 -26.67 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 /D3))
    (pad D2 thru_hole circle (at -7.62 -29.21 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 /D2))
    (pad GND1 thru_hole circle (at -7.62 -31.75 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad RST1 thru_hole circle (at -7.62 -34.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 88 /Reset1))
    (pad D0 thru_hole circle (at -7.62 -36.83 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 /D0))
    (pad D1 thru_hole rect (at -7.62 -39.37 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 /D1))
  )
  (module Pin_Headers:Pin_Header_Straight_1x15_Pitch2.54mm (layer F.Cu) (tedit 5AE975C4)
    (at 146.05 97.155 270)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 270) (layer F.Fab))
    (fp_text value Header1 (at 0 37.89 270) (layer F.Fab))
    (fp_text user %R (at 0 17.78 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 /D1))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 /D0))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 /Reset1))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 /D2))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 /D3))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 /D4))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 /D5))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 /D6))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 /D7))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 /D8))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 /D9))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 /D10))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 /D11))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 /D12))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x15_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15_Pitch2.54mm (layer F.Cu) (tedit 5AE975CA)
    (at 146.05 120.015 270)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 270) (layer F.Fab))
    (fp_text value Header2 (at 0 37.89 270) (layer F.Fab))
    (fp_text user %R (at 0 17.78 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 /Reset2))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A7))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A6))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /A3))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A2))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A1))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A0))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 /AREF))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 /3V3))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 /D13))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x15_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 99.695 (width 0.3) (layer F.Fab)
    (gr_text "99.695 mm" (at 108.2675 29.925) (layer F.Fab))
    (feature1 (pts (xy 158.115 27.305) (xy 158.115 31.275)))
    (feature2 (pts (xy 58.42 27.305) (xy 58.42 31.275)))
    (crossbar (pts (xy 58.42 28.575) (xy 158.115 28.575)))
    (arrow1a (pts (xy 158.115 28.575) (xy 156.988496 29.161421)))
    (arrow1b (pts (xy 158.115 28.575) (xy 156.988496 27.988579)))
    (arrow2a (pts (xy 58.42 28.575) (xy 59.546504 29.161421)))
    (arrow2b (pts (xy 58.42 28.575) (xy 59.546504 27.988579)))
  )
  (dimension 99.695 (width 0.3) (layer F.Fab)
    (gr_text "99.695 mm" (at 161.21 80.9625 270) (layer F.Fab))
    (feature1 (pts (xy 163.83 130.81) (xy 159.86 130.81)))
    (feature2 (pts (xy 163.83 31.115) (xy 159.86 31.115)))
    (crossbar (pts (xy 162.56 31.115) (xy 162.56 130.81)))
    (arrow1a (pts (xy 162.56 130.81) (xy 161.973579 129.683496)))
    (arrow1b (pts (xy 162.56 130.81) (xy 163.146421 129.683496)))
    (arrow2a (pts (xy 162.56 31.115) (xy 161.973579 32.241504)))
    (arrow2b (pts (xy 162.56 31.115) (xy 163.146421 32.241504)))
  )
  (gr_text "(5V tolerant)" (at 86.995 41.91) (layer F.SilkS))
  (gr_text B12 (at 80.01 37.465 90) (layer F.SilkS))
  (gr_text B5 (at 152.4 69.85) (layer F.SilkS))
  (gr_text B4 (at 152.4 67.31) (layer F.SilkS))
  (gr_text A0 (at 147.32 37.465 90) (layer F.SilkS))
  (gr_text A1 (at 144.78 37.465 90) (layer F.SilkS))
  (gr_text A2 (at 142.24 37.465 90) (layer F.SilkS))
  (gr_text A3 (at 139.7 37.465 90) (layer F.SilkS))
  (gr_text A4 (at 137.16 37.465 90) (layer F.SilkS))
  (gr_text A5 (at 134.62 37.465 90) (layer F.SilkS))
  (gr_text A6 (at 132.08 37.465 90) (layer F.SilkS))
  (gr_text A7 (at 129.54 37.465 90) (layer F.SilkS))
  (gr_text B13 (at 82.55 37.465 90) (layer F.SilkS))
  (gr_text B9 (at 97.79 37.465 90) (layer F.SilkS))
  (gr_text B8 (at 95.25 37.465 90) (layer F.SilkS))
  (gr_text A8 (at 92.71 37.465 90) (layer F.SilkS))
  (gr_text A15 (at 90.17 37.465 90) (layer F.SilkS))
  (gr_text A12 (at 87.63 37.465 90) (layer F.SilkS))
  (gr_text A11 (at 85.09 37.465 90) (layer F.SilkS))
  (gr_text "SCK2 (B13)" (at 87.63 74.295 90) (layer F.SilkS))
  (gr_text "MISO2 (B14)" (at 85.09 74.295 90) (layer F.SilkS))
  (gr_text "MOSI2 (B15)" (at 82.55 74.295 90) (layer F.SilkS))
  (gr_text B12 (at 80.01 74.295 90) (layer F.SilkS))
  (gr_text "SDA2 (B11)" (at 77.47 74.295 90) (layer F.SilkS))
  (gr_text "SCL2 (B10)" (at 74.93 74.295 90) (layer F.SilkS))
  (gr_text "TX2 (A2)" (at 72.39 74.295 90) (layer F.SilkS))
  (gr_text "RX2 (A3)" (at 69.85 74.295 90) (layer F.SilkS))
  (gr_text "SCK1 (A5)" (at 137.16 74.295 90) (layer F.SilkS))
  (gr_text "MISO1 (A6)" (at 134.62 74.295 90) (layer F.SilkS))
  (gr_text "MOSI1 (A7)" (at 132.08 74.295 90) (layer F.SilkS))
  (gr_text A4 (at 129.54 74.295 90) (layer F.SilkS))
  (gr_text "SDA1 (B7)" (at 127 74.295 90) (layer F.SilkS))
  (gr_text "SCL1 (B6)" (at 124.46 74.295 90) (layer F.SilkS))
  (gr_text "TX1 (A9)" (at 121.92 74.295 90) (layer F.SilkS))
  (gr_text "RX1 (A10)" (at 119.38 74.295 90) (layer F.SilkS))
  (gr_text C15 (at 152.4 57.15) (layer F.SilkS))
  (gr_text C14 (at 152.4 54.61) (layer F.SilkS))
  (gr_text C13 (at 152.4 52.07) (layer F.SilkS))
  (gr_text B3 (at 152.4 64.77) (layer F.SilkS))
  (gr_text OTHER (at 73.66 38.735) (layer F.SilkS))
  (gr_text ANALOG (at 123.19 38.735) (layer F.SilkS))
  (gr_text "SERIAL 1" (at 144.145 73.66) (layer F.SilkS))
  (gr_text "SERIAL 2" (at 94.615 73.66) (layer F.SilkS))
  (gr_text "Blue Pill v1.0\nnickthecoder.co.uk" (at 81.915 55.88) (layer F.SilkS))
  (gr_text B1 (at 152.4 62.23) (layer F.SilkS))
  (gr_text B0 (at 152.4 59.69) (layer F.SilkS))
  (gr_text DIGITAL (at 150.495 45.085 90) (layer F.SilkS))
  (gr_text Passthrough (at 106.045 95.885 90) (layer B.SilkS))
  (gr_text Enable (at 102.235 95.885 90) (layer B.SilkS))
  (gr_text GND (at 64.77 94.615 90) (layer F.SilkS))
  (gr_text VCC (at 101.6 92.075 90) (layer F.SilkS))
  (gr_text VIN (at 64.77 89.535 90) (layer F.SilkS))
  (gr_text "Prototype v1.0" (at 77.47 82.55) (layer F.SilkS))
  (gr_text http://nickthecoder.co.uk (at 74.295 129.54) (layer F.SilkS))
  (gr_text "Arduino Nano v1.0\nnickthecoder.co.uk" (at 129.54 108.585) (layer F.SilkS))
  (gr_text USB (at 111.76 108.585 90) (layer F.SilkS))
  (gr_text A7 (at 137.16 123.825) (layer F.SilkS))
  (gr_text A6 (at 134.62 123.825) (layer F.SilkS))
  (gr_text ANALOG (at 144.145 123.825) (layer F.SilkS))
  (gr_text "MISO (D12)" (at 132.08 87.63 270) (layer F.SilkS))
  (gr_text A0 (at 119.38 123.825) (layer F.SilkS))
  (gr_text A1 (at 121.92 123.825) (layer F.SilkS))
  (gr_text A5 (at 132.08 123.825) (layer F.SilkS))
  (gr_text A4 (at 129.54 123.825) (layer F.SilkS))
  (gr_text A3 (at 127 123.825) (layer F.SilkS))
  (gr_text A2 (at 124.46 123.825) (layer F.SilkS))
  (gr_text "SCK (D13)" (at 129.54 87.63 270) (layer F.SilkS))
  (gr_text "RXD (D0)" (at 147.32 87.63 270) (layer F.SilkS))
  (gr_text "SCL (A5)" (at 142.24 87.63 270) (layer F.SilkS))
  (gr_text "SDA (A4)" (at 139.7 87.63 270) (layer F.SilkS))
  (gr_text "TXD (D1)" (at 144.78 87.63 270) (layer F.SilkS))
  (gr_text D10 (at 137.16 87.63 270) (layer F.SilkS))
  (gr_text "MOSI (D11)" (at 134.62 87.63 270) (layer F.SilkS))
  (gr_text D9 (at 151.13 120.015) (layer F.SilkS))
  (gr_text D8 (at 151.13 117.475) (layer F.SilkS))
  (gr_text D7 (at 151.13 114.935) (layer F.SilkS))
  (gr_text D6 (at 151.13 112.395) (layer F.SilkS))
  (gr_text D5 (at 151.13 109.855) (layer F.SilkS))
  (gr_text D4 (at 151.13 107.315) (layer F.SilkS))
  (gr_text D3 (at 151.13 104.775) (layer F.SilkS))
  (gr_text D2 (at 151.13 102.235) (layer F.SilkS))
  (gr_text SERIAL (at 121.285 88.265) (layer F.SilkS))
  (gr_text DIGITAL (at 151.13 95.885 90) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer Edge.Cuts) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.001)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.115 130.81) (xy 58.42 130.81) (xy 58.42 31.115) (xy 158.115 31.115)
      )
    )
  )
  (zone (net 9) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.845 79.375) (xy 59.69 79.375) (xy 59.69 32.385) (xy 156.845 32.385)
      )
    )
  )
  (zone (net 39) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.68 129.54) (xy 59.69 129.54) (xy 59.69 82.55) (xy 106.68 82.55)
      )
    )
  )
  (zone (net 39) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.68 129.54) (xy 59.69 129.54) (xy 59.69 82.55) (xy 106.68 82.55)
      )
    )
  )
  (zone (net 9) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.845 129.54) (xy 109.855 129.54) (xy 109.855 82.55) (xy 156.845 82.55)
      )
    )
  )
)
