(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1~bpo9+1)
  (general
    (links 64)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 31)
    (tracks 159)
    (zones 0)
    (modules 10)
    (nets 30)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /A5)
  (net 2 /A4)
  (net 3 /VCC)
  (net 4 /VIN)
  (net 5 /GND)
  (net 6 /D13)
  (net 7 /D12)
  (net 8 /D11)
  (net 9 /D10)
  (net 10 /D1)
  (net 11 /D0)
  (net 12 /D2)
  (net 13 /D3)
  (net 14 /D4)
  (net 15 /D5)
  (net 16 /D6)
  (net 17 /D7)
  (net 18 /D8)
  (net 19 /D9)
  (net 20 /A0)
  (net 21 /A1)
  (net 22 /A2)
  (net 23 /A3)
  (net 24 /A7)
  (net 25 /A6)
  (net 26 /AREF)
  (net 27 /3V3)
  (net 28 /Reset1)
  (net 29 /Reset2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V3)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /AREF)
    (add_net /D0)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /GND)
    (add_net /Reset1)
    (add_net /Reset2)
    (add_net /VCC)
    (add_net /VIN)
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE77EE6)
    (at 119.38 34.925 90)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O1 (at 0 -2.33 90) (layer F.Fab))
    (fp_text value SerialOutput (at 2.54 17.145 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /D13))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D12))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /D11))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /D10))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /D1))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /D0))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE77EFD)
    (at 154.305 41.91)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O2 (at 0 -2.33) (layer F.Fab))
    (fp_text value Output (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /D2))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /D3))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /D4))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /D5))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /D6))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /D7))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /D8))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /D9))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5AE77EF3)
    (at 147.32 76.835 270)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O3 (at 0 -2.33 270) (layer F.Fab))
    (fp_text value Output (at 0 30.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /A7))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /A6))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /A3))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /A2))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /A1))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /A0))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AE88C50)
    (at 154.305 34.925)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference X (at 0 0) (layer F.Fab))
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC36F82)
    (at 154.305 76.835)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.Fab))
    (fp_text value M3 (at 0 -2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC36FB5)
    (at 112.395 76.835)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.Fab))
    (fp_text value M3 (at 0 -2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AE88C5A)
    (at 112.395 34.925)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference X (at 0 0) (layer F.Fab))
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Arduino:Arduino_Nano (layer F.Cu) (tedit 5A860395)
    (at 106.68 58.42 270)
    (descr https://store.arduino.cc/arduino-nano)
    (fp_text reference XA1 (at 6.604 1.016 270) (layer F.Fab))
    (fp_text value Arduino_Nano_Socket (at 0 -21.082 360) (layer F.Fab))
    (fp_text user USB (at 0 0.635 270) (layer F.Fab))
    (fp_text user 3.3V (at 6.35 -6.35 360) (layer F.Fab))
    (fp_text user ICSP (at 0 -40.64 270) (layer F.Fab))
    (pad VIN thru_hole circle (at 7.62 -39.37 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /VIN))
    (pad GND2 thru_hole circle (at 7.62 -36.83 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad RST2 thru_hole circle (at 7.62 -34.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /Reset2))
    (pad 5V thru_hole circle (at 7.62 -31.75 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad A7 thru_hole circle (at 7.62 -29.21 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /A7))
    (pad A6 thru_hole circle (at 7.62 -26.67 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /A6))
    (pad A5 thru_hole circle (at 7.62 -24.13 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad A4 thru_hole circle (at 7.62 -21.59 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad A3 thru_hole circle (at 7.62 -19.05 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /A3))
    (pad A2 thru_hole circle (at 7.62 -16.51 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /A2))
    (pad A1 thru_hole circle (at 7.62 -13.97 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /A1))
    (pad A0 thru_hole circle (at 7.62 -11.43 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /A0))
    (pad AREF thru_hole circle (at 7.62 -8.89 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /AREF))
    (pad 3V3 thru_hole circle (at 7.62 -6.35 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /3V3))
    (pad D13 thru_hole circle (at 7.62 -3.81 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /D13))
    (pad D12 thru_hole circle (at -7.62 -3.81 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /D12))
    (pad D11 thru_hole circle (at -7.62 -6.35 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /D11))
    (pad D10 thru_hole circle (at -7.62 -8.89 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /D10))
    (pad D9 thru_hole circle (at -7.62 -11.43 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /D9))
    (pad D8 thru_hole circle (at -7.62 -13.97 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /D8))
    (pad D7 thru_hole circle (at -7.62 -16.51 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /D7))
    (pad D6 thru_hole circle (at -7.62 -19.05 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /D6))
    (pad D5 thru_hole circle (at -7.62 -21.59 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /D5))
    (pad D4 thru_hole circle (at -7.62 -24.13 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /D4))
    (pad D3 thru_hole circle (at -7.62 -26.67 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /D3))
    (pad D2 thru_hole circle (at -7.62 -29.21 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /D2))
    (pad GND1 thru_hole circle (at -7.62 -31.75 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad RST1 thru_hole circle (at -7.62 -34.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /Reset1))
    (pad D0 thru_hole circle (at -7.62 -36.83 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /D0))
    (pad D1 thru_hole rect (at -7.62 -39.37 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /D1))
  )
  (module Pin_Headers:Pin_Header_Straight_1x15_Pitch2.54mm (layer F.Cu) (tedit 5AE975C4)
    (at 146.05 46.99 270)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 270) (layer F.Fab))
    (fp_text value Header1 (at 0 37.89 270) (layer F.Fab))
    (fp_text user %R (at 0 17.78 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /D1))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /D0))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /Reset1))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /D2))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /D3))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /D4))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /D5))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /D6))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /D7))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /D8))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /D9))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /D10))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /D11))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D12))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x15_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15_Pitch2.54mm (layer F.Cu) (tedit 5AE975CA)
    (at 146.05 69.85 270)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 270) (layer F.Fab))
    (fp_text value Header2 (at 0 37.89 270) (layer F.Fab))
    (fp_text user %R (at 0 17.78 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /Reset2))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /A7))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /A6))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /A5))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /A4))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /A3))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /A2))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /A1))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /A0))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /AREF))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /3V3))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /D13))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x15_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text S (at 129.54 71.755) (layer F.SilkS))
  (gr_text S (at 132.08 71.755) (layer F.SilkS))
  (gr_text "Arduino Nano v1.0\nnickthecoder.co.uk" (at 129.54 58.42) (layer F.SilkS))
  (gr_text USB (at 111.76 58.42 90) (layer F.SilkS))
  (gr_text A7 (at 137.16 73.66) (layer F.SilkS))
  (gr_text A6 (at 134.62 73.66) (layer F.SilkS))
  (gr_text ANALOG (at 144.145 73.66) (layer F.SilkS))
  (gr_text "MISO (D12)" (at 132.08 37.465 270) (layer F.SilkS))
  (gr_text A0 (at 119.38 73.66) (layer F.SilkS))
  (gr_text A1 (at 121.92 73.66) (layer F.SilkS))
  (gr_text A5 (at 132.08 73.66) (layer F.SilkS))
  (gr_text A4 (at 129.54 73.66) (layer F.SilkS))
  (gr_text A3 (at 127 73.66) (layer F.SilkS))
  (gr_text A2 (at 124.46 73.66) (layer F.SilkS))
  (gr_text "SCK (D13)" (at 129.54 37.465 270) (layer F.SilkS))
  (gr_text "RXD (D0)" (at 147.32 37.465 270) (layer F.SilkS))
  (gr_text "SCL (A5)" (at 142.24 37.465 270) (layer F.SilkS))
  (gr_text "SDA (A4)" (at 139.7 37.465 270) (layer F.SilkS))
  (gr_text "TXD (D1)" (at 144.78 37.465 270) (layer F.SilkS))
  (gr_text D10 (at 137.16 37.465 270) (layer F.SilkS))
  (gr_text "MOSI (D11)" (at 134.62 37.465 270) (layer F.SilkS))
  (gr_text D9 (at 151.13 69.85) (layer F.SilkS))
  (gr_text D8 (at 151.13 67.31) (layer F.SilkS))
  (gr_text D7 (at 151.13 64.77) (layer F.SilkS))
  (gr_text D6 (at 151.13 62.23) (layer F.SilkS))
  (gr_text D5 (at 151.13 59.69) (layer F.SilkS))
  (gr_text D4 (at 151.13 57.15) (layer F.SilkS))
  (gr_text D3 (at 151.13 54.61) (layer F.SilkS))
  (gr_text D2 (at 151.13 52.07) (layer F.SilkS))
  (gr_text SERIAL (at 121.285 38.1) (layer F.SilkS))
  (gr_text DIGITAL (at 151.13 45.72 90) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer Edge.Cuts) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.001)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.115 80.645) (xy 108.585 80.645) (xy 108.585 31.115) (xy 158.115 31.115)
      )
    )
  )
  (zone (net 5) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.845 79.375) (xy 109.855 79.375) (xy 109.855 32.385) (xy 156.845 32.385)
      )
    )
  )
)
