(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1~bpo9+1)
  (general
    (links 59)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 7)
    (tracks 107)
    (zones 0)
    (modules 31)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VIN)
  (net 2 /VCC)
  (net 3 /L0)
  (net 4 /L1)
  (net 5 /L2)
  (net 6 /L3)
  (net 7 /L4)
  (net 8 /L5)
  (net 9 /L6)
  (net 10 /L7)
  (net 11 "Net-(D2-Pad1)")
  (net 12 "Net-(D2-Pad2)")
  (net 13 "Net-(D3-Pad1)")
  (net 14 "Net-(D3-Pad2)")
  (net 15 "Net-(D4-Pad1)")
  (net 16 "Net-(D4-Pad2)")
  (net 17 "Net-(D5-Pad1)")
  (net 18 "Net-(D5-Pad2)")
  (net 19 "Net-(D6-Pad1)")
  (net 20 "Net-(D6-Pad2)")
  (net 21 "Net-(D7-Pad1)")
  (net 22 "Net-(D7-Pad2)")
  (net 23 "Net-(D8-Pad1)")
  (net 24 "Net-(D8-Pad2)")
  (net 25 "Net-(D9-Pad1)")
  (net 26 "Net-(D9-Pad2)")
  (net 27 /D0)
  (net 28 /D1)
  (net 29 /D2)
  (net 30 /D3)
  (net 31 /D4)
  (net 32 /D5)
  (net 33 /D6)
  (net 34 /D7)
  (net 35 /VIN2)
  (net 36 /VCC2)
  (net 37 /GND2)
  (net 38 "Net-(D10-Pad2)")
  (net 39 "Net-(J2-Pad2)")
  (net 40 /POWER)
  (net 41 /GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /GND)
    (add_net /GND2)
    (add_net /L0)
    (add_net /L1)
    (add_net /L2)
    (add_net /L3)
    (add_net /L4)
    (add_net /L5)
    (add_net /L6)
    (add_net /L7)
    (add_net /POWER)
    (add_net /VCC)
    (add_net /VCC2)
    (add_net /VIN)
    (add_net /VIN2)
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(J2-Pad2)")
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC3E0E7)
    (at 128.27 128.27)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC3E0E2)
    (at 145.415 128.27)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.Fab))
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC3F278)
    (at 128.27 86.36)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference M3 (at 0 2.54) (layer F.Fab))
    (fp_text value "" (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC3F27C)
    (at 170.18 86.36)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference M3 (at 0 2.54) (layer F.Fab))
    (fp_text value "" (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC3E0EB)
    (at 170.18 128.27)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 128.27 93.345)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference I1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Input (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /L0))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /L1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /L2))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /L3))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /L4))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /L5))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /L6))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /L7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 145.415 93.345)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Output (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /L0))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /L1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /L2))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /L3))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /L4))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /L5))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /L6))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /L7))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Connectors:BARREL_JACK (layer F.Cu) (tedit 5AC3E070)
    (at 137.16 92.71 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J1 (at -8.45 5.75 450) (layer F.SilkS))
    (fp_text value Jack (at -6.2 -5.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 40 /POWER))
    (pad 2 thru_hole rect (at -6 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 41 /GND))
    (pad 3 thru_hole rect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC3E03B)
    (at 145.415 86.36)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.Fab))
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC3E0FE)
    (at 153.035 86.36)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.Fab))
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AC3E0E0)
    (at 153.035 128.27)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.Fab))
    (fp_text value M3 (at 0 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module LEDs:LED_Rectangular_W3.0mm_H2.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 164.465 103.505 180)
    (descr "LED_Rectangular, Rectangular,  Rectangular size 3.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf")
    (tags "LED_Rectangular Rectangular  Rectangular size 3.0x2.0mm^2 2 pins")
    (fp_text reference D2 (at 1.27 -2.06 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.06 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_Rectangular_W3.0mm_H2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_Rectangular_W3.0mm_H2.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 164.465 106.045 180)
    (descr "LED_Rectangular, Rectangular,  Rectangular size 3.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf")
    (tags "LED_Rectangular Rectangular  Rectangular size 3.0x2.0mm^2 2 pins")
    (fp_text reference D3 (at 1.27 -2.06 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.06 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_Rectangular_W3.0mm_H2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_Rectangular_W3.0mm_H2.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 164.465 108.585 180)
    (descr "LED_Rectangular, Rectangular,  Rectangular size 3.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf")
    (tags "LED_Rectangular Rectangular  Rectangular size 3.0x2.0mm^2 2 pins")
    (fp_text reference D4 (at 1.27 -2.06 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.06 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_Rectangular_W3.0mm_H2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_Rectangular_W3.0mm_H2.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 164.465 111.125 180)
    (descr "LED_Rectangular, Rectangular,  Rectangular size 3.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf")
    (tags "LED_Rectangular Rectangular  Rectangular size 3.0x2.0mm^2 2 pins")
    (fp_text reference D5 (at 1.27 -2.06 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.06 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_Rectangular_W3.0mm_H2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_Rectangular_W3.0mm_H2.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 164.465 113.665 180)
    (descr "LED_Rectangular, Rectangular,  Rectangular size 3.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf")
    (tags "LED_Rectangular Rectangular  Rectangular size 3.0x2.0mm^2 2 pins")
    (fp_text reference D6 (at 1.27 -2.06 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.06 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_Rectangular_W3.0mm_H2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_Rectangular_W3.0mm_H2.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 164.465 116.205 180)
    (descr "LED_Rectangular, Rectangular,  Rectangular size 3.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf")
    (tags "LED_Rectangular Rectangular  Rectangular size 3.0x2.0mm^2 2 pins")
    (fp_text reference D7 (at 1.27 -2.06 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.06 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(D7-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_Rectangular_W3.0mm_H2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_Rectangular_W3.0mm_H2.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 164.465 118.745 180)
    (descr "LED_Rectangular, Rectangular,  Rectangular size 3.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf")
    (tags "LED_Rectangular Rectangular  Rectangular size 3.0x2.0mm^2 2 pins")
    (fp_text reference D8 (at 1.27 -2.06 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.06 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "Net-(D8-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_Rectangular_W3.0mm_H2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_Rectangular_W3.0mm_H2.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 164.465 121.285 180)
    (descr "LED_Rectangular, Rectangular,  Rectangular size 3.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf")
    (tags "LED_Rectangular Rectangular  Rectangular size 3.0x2.0mm^2 2 pins")
    (fp_text reference D9 (at 1.27 -2.06 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.06 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(D9-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_Rectangular_W3.0mm_H2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 152.908 93.345)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference I2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Input (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /VIN2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /VCC2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /GND2))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /D0))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /D1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /D2))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /D3))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /D4))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /D5))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /D6))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /D7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 170.18 93.345)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference O2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Output (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /VIN2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /VCC2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /GND2))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /D0))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /D1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /D2))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /D3))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /D4))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /D5))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /D6))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /D7))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Resistors_THT:R_Array_SIP9 (layer F.Cu) (tedit 57FA3974)
    (at 167.64 100.965 270)
    (descr "9-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 11.43 -2.4 270) (layer F.SilkS))
    (fp_text value R_Network08 (at 11.43 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(D2-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D3-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(D5-Pad1)"))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(D6-Pad1)"))
    (pad 7 thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(D7-Pad1)"))
    (pad 8 thru_hole oval (at 17.78 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(D8-Pad1)"))
    (pad 9 thru_hole oval (at 20.32 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(D9-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5AC487DD)
    (at 135.636 127.635)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D10 (at 1.27 1.27) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 /GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AC487BC)
    (at 133.096 120.015)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 3.81 0) (layer F.SilkS))
    (fp_text value R (at 3.81 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 /VIN))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 38 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module eplay:SW_SPDT_8mm (layer F.Cu) (tedit 5932DAF9)
    (at 134.366 111.125)
    (descr "Push switch")
    (tags "switch DPDT")
    (fp_text reference SW1 (at 2.5 1.6) (layer F.SilkS))
    (fp_text value SW_SPST (at 2.5 3.3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 /VIN))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 /POWER))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 0 5.08) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 2.54 5.08) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 5.08 5.08) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask))
  )
  (module Connectors:PINTST (layer F.Cu) (tedit 5AC4A529)
    (at 140.716 123.825)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP1 (at 0 1.905) (layer F.Fab))
    (fp_text value VIN (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 1 /VIN))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST (layer F.Cu) (tedit 5AC4A524)
    (at 133.096 123.825)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP2 (at 0 1.905) (layer F.Fab))
    (fp_text value GND (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 41 /GND))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5AC4AAE7)
    (at 163.195 97.155)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J2 (at -1.7 0 90) (layer F.Fab))
    (fp_text value GS3 (at 1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 36 /VCC2))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at 0 1.27) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 37 /GND2))
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Philmore_TB132_02x5mm_Straight (layer F.Cu) (tedit 5AC4D7BE)
    (at 136.525 104.14 90)
    (descr "2-way 5.0mm pitch terminal block, http://www.philmore-datak.com/mc/Page%20197.pdf")
    (tags "screw terminal block")
    (fp_text reference J3 (at 2.54 1.905 90) (layer F.SilkS))
    (fp_text value Term (at 2.5 6.9 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0.3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.47) (layers *.Cu *.Mask)
      (net 41 /GND))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.47) (layers *.Cu *.Mask)
      (net 40 /POWER))
    (model ${KISYS3DMOD}/Connectors_Terminal_Blocks.3dshapes/TerminalBlock_Philmore_TB132_02x5mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 156.845 103.505)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Choice (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /D0))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /D1))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /D2))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /D3))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /D4))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /D5))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /D6))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /D7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 159.385 103.505)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Select (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(D4-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(D5-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(D6-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(D7-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(D8-Pad2)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text VCC (at 160.02 95.885) (layer F.SilkS))
  (gr_text GND (at 160.02 98.425) (layer F.SilkS))
  (gr_text VIN (at 140.716 125.73) (layer F.SilkS))
  (gr_text GND (at 133.096 125.73) (layer F.SilkS))
  (gr_text "LED Module V1.0\nhttp://nickthecoder.co.uk" (at 157.48 119.38 270) (layer B.SilkS))
  (gr_text "Power Module V1.0\nhttp://nickthecoder.co.uk" (at 138.43 120.015 270) (layer B.SilkS))
  (zone (net 0) (net_name "") (layer Edge.Cuts) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.001)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.99 132.08) (xy 124.46 132.08) (xy 124.46 82.55) (xy 173.99 82.55)
      )
    )
  )
  (zone (net 37) (net_name /GND2) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.72 130.81) (xy 150.495 130.81) (xy 150.495 83.82) (xy 172.72 83.82)
      )
    )
  )
  (zone (net 41) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.955 130.81) (xy 125.73 130.81) (xy 125.73 83.82) (xy 147.955 83.82)
      )
    )
  )
)
